**Question 4**

Interrupts in xv6 are managed by the processor calling a specific interrupt service routine (ISR). The necessary actions are performed by the ISR before returning control to the interrupted process.

System calls in xv6 are managed through executing the interrupt instruction of a specific software, the processor transfers control to the system call handler to perform the actions required before returning control to the software program.